<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="42.182" y2="0" width="0" layer="20"/>
<wire x1="42.182" y1="0" x2="42.182" y2="32.994" width="0" layer="20"/>
<wire x1="42.182" y1="32.994" x2="0" y2="32.994" width="0" layer="20"/>
<wire x1="0" y1="32.994" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="33.324" width="0.8128" layer="46"/>
<wire x1="0" y1="33.324" x2="42.202" y2="33.324" width="0.8128" layer="46"/>
<wire x1="42.202" y1="33.324" x2="42.202" y2="0" width="0.8128" layer="46"/>
<wire x1="42.202" y1="0" x2="0" y2="0" width="0.8128" layer="46"/>
</plain>
<libraries>
<library name="eagle_fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="eagle_fab" package="C1206FAB" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="eagle_fab" package="LED1206FAB" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="eagle_fab" package="1X06SMD" value="FTDI">
<attribute name="NAME"/>
</element>
<element name="R1" library="eagle_fab" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="eagle_fab" package="6MM_SWITCH" value="switch">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="eagle_fab" package="SOIC8" value="UC_ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="eagle_fab" package="2X03SMD" value="CONN_03X2_AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="LED">
<contactref element="U1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="PB">
<contactref element="S1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
